#==================================================================================
#
#                        ==== MergeCOM-3 Service Profile ====
#
#        The location of this file is provided in the MERGECOM_3_SERVICES parameter
#        of the [MergeCOM3] section of the MERGE.INI file.
#
#        This file is GENERATED by the MergeCOM-3 Profile Database Utilities
#                 DO NOT CHANGE THE CONTENTS OF THIS FILE MANUALLY
#
#==================================================================================
#    This file generated on 11/18/2011 3:20:05 PM
#==================================================================================
#
# Contains the following sections:
#        [SERVICE_TABLE]     - List of service names and numbers
#        [service_number]    - One section number for each of the above services


#==================================================================================
#                                   Service Table
#                        Service Names to Service Numbers
#==================================================================================
[SERVICE_TABLE]
    NUMBER_OF_SERVICES_SUPPORTED          = 201
    ARTERIAL_PULSE_WAVEFORM               = 0001
    AUTOREFRACTION_MEASUREMENTS           = 0002
    BASIC_ANNOTATION_BOX                  = 0003
    BASIC_COLOR_IMAGE_BOX                 = 0004
    BASIC_FILM_BOX                        = 0005
    BASIC_FILM_SESSION                    = 0006
    BASIC_GRAYSCALE_IMAGE_BOX             = 0007
    BASIC_PRINT_IMAGE_OVERLAY_BOX         = 0008
    BASIC_STRUCTURED_DISPLAY              = 0009
    BREAST_IMAGING_RPI_QUERY              = 0010
    BREAST_TOMO_IMAGE_STORAGE             = 0011
    CARDIAC_RPI_QUERY                     = 0012
    CHEST_CAD_SR                          = 0013
    COLON_CAD_SR                          = 0014
    COLOR_PALETTE_FIND                    = 0015
    COLOR_PALETTE_GET                     = 0016
    COLOR_PALETTE_MOVE                    = 0017
    COLOR_PALETTE_STORAGE                 = 0018
    COMPOSITE_INST_RET_NO_BULK_GET        = 0019
    COMPOSITE_INSTANCE_ROOT_RET_GET       = 0020
    COMPOSITE_INSTANCE_ROOT_RET_MOVE      = 0021
    DEFORMABLE_SPATIAL_REGISTRATION       = 0022
    DETACHED_INTERP_MANAGEMENT            = 0023
    DETACHED_PATIENT_MANAGEMENT           = 0024
    DETACHED_RESULTS_MANAGEMENT           = 0025
    DETACHED_STUDY_MANAGEMENT             = 0026
    DETACHED_VISIT_MANAGEMENT             = 0027
    DICOMDIR                              = 0028
    ENCAPSULATED_CDA                      = 0029
    ENHANCED_CT_IMAGE                     = 0030
    ENHANCED_MR_COLOR_IMAGE               = 0031
    ENHANCED_MR_IMAGE                     = 0032
    ENHANCED_PET_IMAGE                    = 0033
    ENHANCED_US_VOLUME                    = 0034
    ENHANCED_XA_IMAGE                     = 0035
    ENHANCED_XRF_IMAGE                    = 0036
    G_P_PERFORMED_PROCEDURE_STEP          = 0037
    G_P_SCHEDULED_PROCEDURE_STEP          = 0038
    G_P_WORKLIST                          = 0039
    GENERAL_AUDIO_WAVEFORM                = 0040
    GENERAL_RPI_QUERY                     = 0041
    GENERIC_IMPLANT_TEMPLATE              = 0042
    GENERIC_IMPLANT_TEMPLATE_FIND         = 0043
    GENERIC_IMPLANT_TEMPLATE_GET          = 0044
    GENERIC_IMPLANT_TEMPLATE_MOVE         = 0045
    HANGING_PROTOCOL                      = 0046
    HANGING_PROTOCOL_FIND                 = 0047
    HANGING_PROTOCOL_GET                  = 0048
    HANGING_PROTOCOL_MOVE                 = 0049
    IMAGE_OVERLAY_BOX_RETIRED             = 0050
    IMPLANT_ASSEMBLY_TEMPLATE             = 0051
    IMPLANT_ASSEMBLY_TEMPLATE_FIND        = 0052
    IMPLANT_ASSEMBLY_TEMPLATE_GET         = 0053
    IMPLANT_ASSEMBLY_TEMPLATE_MOVE        = 0054
    IMPLANT_TEMPLATE_GROUP                = 0055
    IMPLANT_TEMPLATE_GROUP_FIND           = 0056
    IMPLANT_TEMPLATE_GROUP_GET            = 0057
    IMPLANT_TEMPLATE_GROUP_MOVE           = 0058
    IMPLANTATION_PLAN_SR_DOCUMENT         = 0059
    INSTANCE_AVAIL_NOTIFICATION           = 0060
    INTRAOCULAR_LENS_CALCULATIONS         = 0061
    KERATOMETRY_MEASUREMENTS              = 0062
    KEY_OBJECT_SELECTION_DOC              = 0063
    LENSOMETRY_MEASUREMENTS               = 0064
    MACULAR_GRID_THIICKNESS_VOLUME        = 0065
    MAMMOGRAPHY_CAD_SR                    = 0066
    MEDIA_CREATION_MANAGEMENT             = 0067
    MODALITY_WORKLIST_FIND                = 0068
    MR_SPECTROSCOPY                       = 0069
    OPHT_VIS_FIELD_STATIC_PERIM_MEAS      = 0070
    OPHTHALMIC_AXIAL_MEASUREMENTS         = 0071
    OPHTHALMIC_TOMOGRAPHY_IMAGE           = 0072
    OPM_THICKNESS_MAP                     = 0073
    PATIENT_ROOT_QR_FIND                  = 0074
    PATIENT_ROOT_QR_GET                   = 0075
    PATIENT_ROOT_QR_MOVE                  = 0076
    PATIENT_STUDY_ONLY_QR_FIND            = 0077
    PATIENT_STUDY_ONLY_QR_GET             = 0078
    PATIENT_STUDY_ONLY_QR_MOVE            = 0079
    PERFORMED_PROCEDURE_STEP              = 0080
    PERFORMED_PROCEDURE_STEP_NOTIFY       = 0081
    PERFORMED_PROCEDURE_STEP_RETR         = 0082
    PRESENTATION_LUT                      = 0083
    PRINT_JOB                             = 0084
    PRINT_QUEUE_MANAGEMENT                = 0085
    PRINTER                               = 0086
    PRINTER_CONFIGURATION                 = 0087
    PROCEDURAL_EVENT_LOGGING              = 0088
    PROCEDURE_LOG                         = 0089
    PRODUCT_CHARACTERISTICS_QUERY         = 0090
    PULL_PRINT_REQUEST                    = 0091
    RAW_DATA                              = 0092
    REAL_WORLD_VALUE_MAPPING              = 0093
    REFERENCED_IMAGE_BOX                  = 0094
    RESPIRATORY_WAVEFORM                  = 0095
    RT_BEAMS_DELIVERY_INSTRUCTION         = 0096
    RT_CONVENTIONAL_MACHINE_VERIF         = 0097
    RT_ION_MACHINE_VERIF                  = 0098
    SC_MULTIFRAME_GRAYSCALE_BYTE          = 0099
    SC_MULTIFRAME_GRAYSCALE_WORD          = 0100
    SC_MULTIFRAME_SINGLE_BIT              = 0101
    SC_MULTIFRAME_TRUE_COLOR              = 0102
    SEGMENTATION                          = 0103
    SPATIAL_FIDUCIALS                     = 0104
    SPATIAL_REGISTRATION                  = 0105
    SPECTACLE_PRESCRIPTION_REPORT         = 0106
    STANDARD_BASIC_TEXT_SR                = 0107
    STANDARD_BLENDING_SOFTCOPY_PS         = 0108
    STANDARD_COLOR_SOFTCOPY_PS            = 0109
    STANDARD_COMPREHENSIVE_SR             = 0110
    STANDARD_CR                           = 0111
    STANDARD_CT                           = 0112
    STANDARD_CURVE                        = 0113
    STANDARD_DX_PRESENT                   = 0114
    STANDARD_DX_PROCESS                   = 0115
    STANDARD_ECHO                         = 0116
    STANDARD_ENCAPSULATED_PDF             = 0117
    STANDARD_ENHANCED_SR                  = 0118
    STANDARD_GRAYSCALE_SOFTCOPY_PS        = 0119
    STANDARD_HARDCOPY_COLOR               = 0120
    STANDARD_HARDCOPY_GRAYSCALE           = 0121
    STANDARD_IO_PRESENT                   = 0122
    STANDARD_IO_PROCESS                   = 0123
    STANDARD_IVOCT_PRESENT                = 0124
    STANDARD_IVOCT_PROCESS                = 0125
    STANDARD_MG_PRESENT                   = 0126
    STANDARD_MG_PROCESS                   = 0127
    STANDARD_MODALITY_LUT                 = 0128
    STANDARD_MR                           = 0129
    STANDARD_NM                           = 0130
    STANDARD_NM_RETIRED                   = 0131
    STANDARD_OPHTHALMIC_16_BIT            = 0132
    STANDARD_OPHTHALMIC_8_BIT             = 0133
    STANDARD_OVERLAY                      = 0134
    STANDARD_PET                          = 0135
    STANDARD_PET_CURVE                    = 0136
    STANDARD_PRINT_STORAGE                = 0137
    STANDARD_PSEUDOCOLOR_SOFTCOPY_PS      = 0138
    STANDARD_RT_BEAMS_TREAT               = 0139
    STANDARD_RT_BRACHY_TREAT              = 0140
    STANDARD_RT_DOSE                      = 0141
    STANDARD_RT_IMAGE                     = 0142
    STANDARD_RT_ION_BEAMS_TREAT           = 0143
    STANDARD_RT_ION_PLAN                  = 0144
    STANDARD_RT_PLAN                      = 0145
    STANDARD_RT_STRUCTURE_SET             = 0146
    STANDARD_RT_TREAT_SUM                 = 0147
    STANDARD_SEC_CAPTURE                  = 0148
    STANDARD_US                           = 0149
    STANDARD_US_MF                        = 0150
    STANDARD_US_MF_RETIRED                = 0151
    STANDARD_US_RETIRED                   = 0152
    STANDARD_VIDEO_ENDOSCOPIC             = 0153
    STANDARD_VIDEO_MICROSCOPIC            = 0154
    STANDARD_VIDEO_PHOTOGRAPHIC           = 0155
    STANDARD_VL_ENDOSCOPIC                = 0156
    STANDARD_VL_MICROSCOPIC               = 0157
    STANDARD_VL_PHOTOGRAPHIC              = 0158
    STANDARD_VL_SLIDE_MICROSCOPIC         = 0159
    STANDARD_VOI_LUT                      = 0160
    STANDARD_WAVEFORM_12_LEAD_ECG         = 0161
    STANDARD_WAVEFORM_AMBULATORY_ECG      = 0162
    STANDARD_WAVEFORM_BASIC_VOICE_AU      = 0163
    STANDARD_WAVEFORM_CARDIAC_EP          = 0164
    STANDARD_WAVEFORM_GENERAL_ECG         = 0165
    STANDARD_WAVEFORM_HEMODYNAMIC         = 0166
    STANDARD_XRAY_ANGIO                   = 0167
    STANDARD_XRAY_ANGIO_BIPLANE           = 0168
    STANDARD_XRAY_RF                      = 0169
    STEREOMETRIC_RELATIONSHIP             = 0170
    STORAGE_COMMITMENT_PULL               = 0171
    STORAGE_COMMITMENT_PUSH               = 0172
    STUDY_COMPONENT_MANAGEMENT            = 0173
    STUDY_CONTENT_NOTIFICATION            = 0174
    STUDY_ROOT_QR_FIND                    = 0175
    STUDY_ROOT_QR_GET                     = 0176
    STUDY_ROOT_QR_MOVE                    = 0177
    SUBJ_REFRACTION_MEASUREMENTS          = 0178
    SUBSTANCE_ADMIN_LOGGING               = 0179
    SUBSTANCE_APPROVAL_QUERY              = 0180
    SURFACE_SEGMENTATION                  = 0181
    UPS_EVENT_SOP                         = 0182
    UPS_PULL_SOP                          = 0183
    UPS_PUSH_SOP                          = 0184
    UPS_WATCH_SOP                         = 0185
    VISUAL_ACUITY_MEASUREMENTS            = 0186
    VL_WHOLE_SLIDE_MICROSCOPY_IMAGE       = 0187
    VOI_LUT_BOX                           = 0188
    XA_XRF_GRAYSCALE_SOFTCOPY_PS          = 0189
    XRAY_3D_ANGIO_IMAGE                   = 0190
    XRAY_3D_CRANIO_IMAGE                  = 0191
    XRAY_RADATION_DOSE_SR                 = 0192
    BASIC_COLOR_PRINT_MANAGEMENT          = 0193
    BASIC_GRAYSCALE_PRINT_MANAGEMENT      = 0194
    DETACHED_PATIENT_MANAGEMENT_META      = 0195
    DETACHED_RESULTS_MANAGEMENT_META      = 0196
    G_P_WORKLIST_MANAGEMENT_META          = 0197
    PULL_STORED_PRINT_MANAGEMENT          = 0198
    REF_COLOR_PRINT_MANAGEMENT            = 0199
    REF_GRAYSCALE_PRINT_MANAGEMENT        = 0200
    STUDY_MANAGEMENT                      = 0201


#==================================================================================
#                             Service Definitions
#                Name, UID, Type (Base or Meta), and DIMSE Services
#==================================================================================
[0001]
        NAME                    = ARTERIAL_PULSE_WAVEFORM
        UID                     = 1.2.840.10008.5.1.4.1.1.9.5.1
        DESCRIPTION             = ARTERIAL PULSE WAVEFORM STORAGE
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0002]
        NAME                    = AUTOREFRACTION_MEASUREMENTS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.2
        DESCRIPTION             = Autorefraction Measurements Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0003]
        NAME                    = BASIC_ANNOTATION_BOX
        UID                     = 1.2.840.10008.5.1.1.15
        DESCRIPTION             = Basic Annotation Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_SET_RQ
        COMMAND_2               = N_SET_RSP


[0004]
        NAME                    = BASIC_COLOR_IMAGE_BOX
        UID                     = 1.2.840.10008.5.1.1.4.1
        DESCRIPTION             = Basic Color Image Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_SET_RQ
        COMMAND_2               = N_SET_RSP


[0005]
        NAME                    = BASIC_FILM_BOX
        UID                     = 1.2.840.10008.5.1.1.2
        DESCRIPTION             = Basic Film Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP
        COMMAND_7               = N_ACTION_RQ
        COMMAND_8               = N_ACTION_RSP


[0006]
        NAME                    = BASIC_FILM_SESSION
        UID                     = 1.2.840.10008.5.1.1.1
        DESCRIPTION             = Basic Film Session SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP
        COMMAND_7               = N_ACTION_RQ
        COMMAND_8               = N_ACTION_RSP


[0007]
        NAME                    = BASIC_GRAYSCALE_IMAGE_BOX
        UID                     = 1.2.840.10008.5.1.1.4
        DESCRIPTION             = Basic Grayscale Image Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_SET_RQ
        COMMAND_2               = N_SET_RSP


[0008]
        NAME                    = BASIC_PRINT_IMAGE_OVERLAY_BOX
        UID                     = 1.2.840.10008.5.1.1.24.1
        DESCRIPTION             = Basic Print Image Overlay Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_SET_RQ
        COMMAND_2               = N_SET_RSP
        COMMAND_3               = N_DELETE_RQ
        COMMAND_4               = N_DELETE_RSP
        COMMAND_5               = N_CREATE_RQ
        COMMAND_6               = N_CREATE_RSP


[0009]
        NAME                    = BASIC_STRUCTURED_DISPLAY
        UID                     = 1.2.840.10008.5.1.4.1.1.131
        DESCRIPTION             = BASIC STRUCTURED DISPLAY SOP STORAGE
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0010]
        NAME                    = BREAST_IMAGING_RPI_QUERY
        UID                     = 1.2.840.10008.5.1.4.37.2
        DESCRIPTION             = Breast Imaging Relevant Patient Information Query
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0011]
        NAME                    = BREAST_TOMO_IMAGE_STORAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.13.1.3
        DESCRIPTION             = BREAST TOMOSYNTHESIS IMAGE SOP CLASS
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0012]
        NAME                    = CARDIAC_RPI_QUERY
        UID                     = 1.2.840.10008.5.1.4.37.3
        DESCRIPTION             = Cardiac Relevant Patient Information Query
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0013]
        NAME                    = CHEST_CAD_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.65
        DESCRIPTION             = Chest CAD SR Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0014]
        NAME                    = COLON_CAD_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.69
        DESCRIPTION             = Colon CAD SR
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0015]
        NAME                    = COLOR_PALETTE_FIND
        UID                     = 1.2.840.10008.5.1.4.39.2
        DESCRIPTION             = Color Palette C-FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0016]
        NAME                    = COLOR_PALETTE_GET
        UID                     = 1.2.840.10008.5.1.4.39.4
        DESCRIPTION             = Color Palette C-GET
        TYPE                    = BASE
        COMMAND_1               = C_GET_RQ
        COMMAND_2               = C_GET_RSP
        COMMAND_3               = C_CANCEL_RQ


[0017]
        NAME                    = COLOR_PALETTE_MOVE
        UID                     = 1.2.840.10008.5.1.4.39.3
        DESCRIPTION             = Color Palette C-MOVE
        TYPE                    = BASE
        COMMAND_1               = C_MOVE_RQ
        COMMAND_2               = C_MOVE_RSP
        COMMAND_3               = C_CANCEL_RQ


[0018]
        NAME                    = COLOR_PALETTE_STORAGE
        UID                     = 1.2.840.10008.5.1.4.39.1
        DESCRIPTION             = Color Palette Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0019]
        NAME                    = COMPOSITE_INST_RET_NO_BULK_GET
        UID                     = 1.2.840.10008.5.1.4.1.2.5.3
        DESCRIPTION             = Composite Instance Retrieve Without Bulk Data - GET
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_GET_RQ
        COMMAND_3               = C_GET_RSP


[0020]
        NAME                    = COMPOSITE_INSTANCE_ROOT_RET_GET
        UID                     = 1.2.840.10008.5.1.4.1.2.4.3
        DESCRIPTION             = Composite Instance Root Retrieve - GET
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_GET_RQ
        COMMAND_3               = C_GET_RSP


[0021]
        NAME                    = COMPOSITE_INSTANCE_ROOT_RET_MOVE
        UID                     = 1.2.840.10008.5.1.4.1.2.4.2
        DESCRIPTION             = Composite Instance Root Retrieve - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_MOVE_RQ
        COMMAND_3               = C_MOVE_RSP


[0022]
        NAME                    = DEFORMABLE_SPATIAL_REGISTRATION
        UID                     = 1.2.840.10008.5.1.4.1.1.66.3
        DESCRIPTION             = Deformable Spatial Registration
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0023]
        NAME                    = DETACHED_INTERP_MANAGEMENT
        UID                     = 1.2.840.10008.3.1.2.6.1
        DESCRIPTION             = Detached Interpretation Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_EVENT_REPORT_RQ
        COMMAND_6               = N_EVENT_REPORT_RSP


[0024]
        NAME                    = DETACHED_PATIENT_MANAGEMENT
        UID                     = 1.2.840.10008.3.1.2.1.1
        DESCRIPTION             = Detached Patient Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP
        COMMAND_3               = N_EVENT_REPORT_RSP
        COMMAND_4               = N_EVENT_REPORT_RQ


[0025]
        NAME                    = DETACHED_RESULTS_MANAGEMENT
        UID                     = 1.2.840.10008.3.1.2.5.1
        DESCRIPTION             = Detached Results Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP
        COMMAND_3               = N_EVENT_REPORT_RSP
        COMMAND_4               = N_EVENT_REPORT_RQ


[0026]
        NAME                    = DETACHED_STUDY_MANAGEMENT
        UID                     = 1.2.840.10008.3.1.2.3.1
        DESCRIPTION             = Detached Study Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_EVENT_REPORT_RSP
        COMMAND_6               = N_EVENT_REPORT_RQ


[0027]
        NAME                    = DETACHED_VISIT_MANAGEMENT
        UID                     = 1.2.840.10008.3.1.2.2.1
        DESCRIPTION             = Detached Visit Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_EVENT_REPORT_RSP
        COMMAND_6               = N_EVENT_REPORT_RQ


[0028]
        NAME                    = DICOMDIR
        UID                     = 1.2.840.10008.1.3.10
        DESCRIPTION             = Media Storage Directory Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ


[0029]
        NAME                    = ENCAPSULATED_CDA
        UID                     = 1.2.840.10008.5.1.4.1.1.104.2
        DESCRIPTION             = Encapsulated CDA Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0030]
        NAME                    = ENHANCED_CT_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.2.1
        DESCRIPTION             = Enhanced CT Image
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0031]
        NAME                    = ENHANCED_MR_COLOR_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.4.3
        DESCRIPTION             = Enhanced MR Color Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0032]
        NAME                    = ENHANCED_MR_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.4.1
        DESCRIPTION             = Enhance MR Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0033]
        NAME                    = ENHANCED_PET_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.130
        DESCRIPTION             = Enhanced PET Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0034]
        NAME                    = ENHANCED_US_VOLUME
        UID                     = 1.2.840.10008.5.1.4.1.1.6.2
        DESCRIPTION             = ENHANCED US VOLUME STORAGE
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0035]
        NAME                    = ENHANCED_XA_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.12.1.1
        DESCRIPTION             = Enhanced XA Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0036]
        NAME                    = ENHANCED_XRF_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.12.2.1
        DESCRIPTION             = Enhanced XRF Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0037]
        NAME                    = G_P_PERFORMED_PROCEDURE_STEP
        UID                     = 1.2.840.10008.5.1.4.32.3
        DESCRIPTION             = General Purpose Performed Procedure Step SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RSP
        COMMAND_2               = N_SET_RSP
        COMMAND_3               = N_CREATE_RSP
        COMMAND_4               = N_SET_RQ
        COMMAND_5               = N_GET_RQ
        COMMAND_6               = N_CREATE_RQ


[0038]
        NAME                    = G_P_SCHEDULED_PROCEDURE_STEP
        UID                     = 1.2.840.10008.5.1.4.32.2
        DESCRIPTION             = General Purpose Scheduled Procedure Step SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_ACTION_RQ
        COMMAND_2               = N_ACTION_RSP


[0039]
        NAME                    = G_P_WORKLIST
        UID                     = 1.2.840.10008.5.1.4.32.1
        DESCRIPTION             = General Purpose Woklist Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0040]
        NAME                    = GENERAL_AUDIO_WAVEFORM
        UID                     = 1.2.840.10008.5.1.4.1.1.9.4.2
        DESCRIPTION             = GENERAL AUDIO WAVEFORM STORAGE
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0041]
        NAME                    = GENERAL_RPI_QUERY
        UID                     = 1.2.840.10008.5.1.4.37.1
        DESCRIPTION             = General Relevant Patient Information Query
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0042]
        NAME                    = GENERIC_IMPLANT_TEMPLATE
        UID                     = 1.2.840.10008.5.1.4.43.1
        DESCRIPTION             = Generic Implant Template Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0043]
        NAME                    = GENERIC_IMPLANT_TEMPLATE_FIND
        UID                     = 1.2.840.10008.5.1.4.43.2
        DESCRIPTION             = Generic Implant Template Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0044]
        NAME                    = GENERIC_IMPLANT_TEMPLATE_GET
        UID                     = 1.2.840.10008.5.1.4.43.4
        DESCRIPTION             = Generic Implant Template Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_GET_RQ
        COMMAND_2               = C_GET_RSP
        COMMAND_3               = C_CANCEL_RQ


[0045]
        NAME                    = GENERIC_IMPLANT_TEMPLATE_MOVE
        UID                     = 1.2.840.10008.5.1.4.43.3
        DESCRIPTION             = Generic Implant Template Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_MOVE_RQ
        COMMAND_2               = C_MOVE_RSP
        COMMAND_3               = C_CANCEL_RQ


[0046]
        NAME                    = HANGING_PROTOCOL
        UID                     = 1.2.840.10008.5.1.4.38.1
        DESCRIPTION             = Hanging Protocol Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0047]
        NAME                    = HANGING_PROTOCOL_FIND
        UID                     = 1.2.840.10008.5.1.4.38.2
        DESCRIPTION             = Hanging Protocol Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0048]
        NAME                    = HANGING_PROTOCOL_GET
        UID                     = 1.2.840.10008.5.1.4.38.4
        DESCRIPTION             = Hanging Protocol Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_GET_RQ
        COMMAND_2               = C_GET_RSP
        COMMAND_3               = C_CANCEL_RQ


[0049]
        NAME                    = HANGING_PROTOCOL_MOVE
        UID                     = 1.2.840.10008.5.1.4.38.3
        DESCRIPTION             = Hanging Protocol Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_MOVE_RQ
        COMMAND_2               = C_MOVE_RSP
        COMMAND_3               = C_CANCEL_RQ


[0050]
        NAME                    = IMAGE_OVERLAY_BOX_RETIRED
        UID                     = 1.2.840.10008.5.1.1.24
        DESCRIPTION             = Image Overlay Box SOP Class Retired
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP


[0051]
        NAME                    = IMPLANT_ASSEMBLY_TEMPLATE
        UID                     = 1.2.840.10008.5.1.4.44.1
        DESCRIPTION             = Implant Assembly Template Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0052]
        NAME                    = IMPLANT_ASSEMBLY_TEMPLATE_FIND
        UID                     = 1.2.840.10008.5.1.4.44.2
        DESCRIPTION             = Implant Assembly Template Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0053]
        NAME                    = IMPLANT_ASSEMBLY_TEMPLATE_GET
        UID                     = 1.2.840.10008.5.1.4.44.4
        DESCRIPTION             = Implant Assembly Template Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_GET_RQ
        COMMAND_2               = C_GET_RSP
        COMMAND_3               = C_CANCEL_RQ


[0054]
        NAME                    = IMPLANT_ASSEMBLY_TEMPLATE_MOVE
        UID                     = 1.2.840.10008.5.1.4.44.3
        DESCRIPTION             = Implant Assembly Template Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_MOVE_RQ
        COMMAND_2               = C_MOVE_RSP
        COMMAND_3               = C_CANCEL_RQ


[0055]
        NAME                    = IMPLANT_TEMPLATE_GROUP
        UID                     = 1.2.840.10008.5.1.4.45.1
        DESCRIPTION             = Implant Template Group Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0056]
        NAME                    = IMPLANT_TEMPLATE_GROUP_FIND
        UID                     = 1.2.840.10008.5.1.4.45.2
        DESCRIPTION             = Implant Template Group Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0057]
        NAME                    = IMPLANT_TEMPLATE_GROUP_GET
        UID                     = 1.2.840.10008.5.1.4.45.4
        DESCRIPTION             = Implant Template Group Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_GET_RQ
        COMMAND_2               = C_GET_RSP
        COMMAND_3               = C_CANCEL_RQ


[0058]
        NAME                    = IMPLANT_TEMPLATE_GROUP_MOVE
        UID                     = 1.2.840.10008.5.1.4.45.3
        DESCRIPTION             = Implant Template Group Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_MOVE_RQ
        COMMAND_2               = C_MOVE_RSP
        COMMAND_3               = C_CANCEL_RQ


[0059]
        NAME                    = IMPLANTATION_PLAN_SR_DOCUMENT
        UID                     = 1.2.840.10008.5.1.4.1.1.88.70
        DESCRIPTION             = Implantation Plan SR Document Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0060]
        NAME                    = INSTANCE_AVAIL_NOTIFICATION
        UID                     = 1.2.840.10008.5.1.4.33
        DESCRIPTION             = Instance Availability Notification
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP


[0061]
        NAME                    = INTRAOCULAR_LENS_CALCULATIONS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.8
        DESCRIPTION             = Intraocular Lens Calculations Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0062]
        NAME                    = KERATOMETRY_MEASUREMENTS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.3
        DESCRIPTION             = Keratometry Measurements Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0063]
        NAME                    = KEY_OBJECT_SELECTION_DOC
        UID                     = 1.2.840.10008.5.1.4.1.1.88.59
        DESCRIPTION             = Key Object Selection Document
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0064]
        NAME                    = LENSOMETRY_MEASUREMENTS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.1
        DESCRIPTION             = Lensometry Measurements Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0065]
        NAME                    = MACULAR_GRID_THIICKNESS_VOLUME
        UID                     = 1.2.840.10008.5.1.4.1.1.79.1
        DESCRIPTION             = Macular Grid Thickness and Volume Report
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0066]
        NAME                    = MAMMOGRAPHY_CAD_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.50
        DESCRIPTION             = Mammography CAD SR SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0067]
        NAME                    = MEDIA_CREATION_MANAGEMENT
        UID                     = 1.2.840.10008.5.1.1.33
        DESCRIPTION             = Media Creation Management
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_ACTION_RQ
        COMMAND_4               = N_ACTION_RSP
        COMMAND_5               = N_GET_RQ
        COMMAND_6               = N_GET_RSP


[0068]
        NAME                    = MODALITY_WORKLIST_FIND
        UID                     = 1.2.840.10008.5.1.4.31
        DESCRIPTION             = Modality Worklist Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = C_CANCEL_RQ


[0069]
        NAME                    = MR_SPECTROSCOPY
        UID                     = 1.2.840.10008.5.1.4.1.1.4.2
        DESCRIPTION             = MR Spectroscopy Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0070]
        NAME                    = OPHT_VIS_FIELD_STATIC_PERIM_MEAS
        UID                     = 1.2.840.10008.5.1.4.1.1.80.1
        DESCRIPTION             = Ophthalmic Visual Field Static Perimetry Measurements Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0071]
        NAME                    = OPHTHALMIC_AXIAL_MEASUREMENTS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.7
        DESCRIPTION             = Ophthalmic Axial Measurements Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0072]
        NAME                    = OPHTHALMIC_TOMOGRAPHY_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.5.4
        DESCRIPTION             = Ophthalmic Tomography Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0073]
        NAME                    = OPM_THICKNESS_MAP
        UID                     = 1.2.840.10008.5.1.4.1.1.81.1
        DESCRIPTION             = Ophthalmic Thickness Map Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0074]
        NAME                    = PATIENT_ROOT_QR_FIND
        UID                     = 1.2.840.10008.5.1.4.1.2.1.1
        DESCRIPTION             = Patient Root Query/Retrieve Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_FIND_RQ
        COMMAND_3               = C_FIND_RSP


[0075]
        NAME                    = PATIENT_ROOT_QR_GET
        UID                     = 1.2.840.10008.5.1.4.1.2.1.3
        DESCRIPTION             = Patient Root Query/Retrieve Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_GET_RQ
        COMMAND_3               = C_GET_RSP


[0076]
        NAME                    = PATIENT_ROOT_QR_MOVE
        UID                     = 1.2.840.10008.5.1.4.1.2.1.2
        DESCRIPTION             = Patient Root Query/Retrieve Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_MOVE_RQ
        COMMAND_3               = C_MOVE_RSP


[0077]
        NAME                    = PATIENT_STUDY_ONLY_QR_FIND
        UID                     = 1.2.840.10008.5.1.4.1.2.3.1
        DESCRIPTION             = Patient/Study Only Query/Retrieve Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_FIND_RQ
        COMMAND_3               = C_FIND_RSP


[0078]
        NAME                    = PATIENT_STUDY_ONLY_QR_GET
        UID                     = 1.2.840.10008.5.1.4.1.2.3.3
        DESCRIPTION             = Patient/Study Only Query/Retrieve Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_GET_RQ
        COMMAND_3               = C_GET_RSP


[0079]
        NAME                    = PATIENT_STUDY_ONLY_QR_MOVE
        UID                     = 1.2.840.10008.5.1.4.1.2.3.2
        DESCRIPTION             = Patient/Study Only Query/Retrieve Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_MOVE_RQ
        COMMAND_3               = C_MOVE_RSP


[0080]
        NAME                    = PERFORMED_PROCEDURE_STEP
        UID                     = 1.2.840.10008.3.1.2.3.3
        DESCRIPTION             = Modality Performed Procedure Step SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP


[0081]
        NAME                    = PERFORMED_PROCEDURE_STEP_NOTIFY
        UID                     = 1.2.840.10008.3.1.2.3.5
        DESCRIPTION             = Modality Performed Procedure Step Notification SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_EVENT_REPORT_RQ
        COMMAND_2               = N_EVENT_REPORT_RSP


[0082]
        NAME                    = PERFORMED_PROCEDURE_STEP_RETR
        UID                     = 1.2.840.10008.3.1.2.3.4
        DESCRIPTION             = Modality Performed Procedure Step Retrieve SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP


[0083]
        NAME                    = PRESENTATION_LUT
        UID                     = 1.2.840.10008.5.1.1.23
        DESCRIPTION             = Presentation LUT SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_DELETE_RQ
        COMMAND_4               = N_DELETE_RSP


[0084]
        NAME                    = PRINT_JOB
        UID                     = 1.2.840.10008.5.1.1.14
        DESCRIPTION             = Print Job SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_EVENT_REPORT_RQ
        COMMAND_2               = N_EVENT_REPORT_RSP
        COMMAND_3               = N_GET_RQ
        COMMAND_4               = N_GET_RSP


[0085]
        NAME                    = PRINT_QUEUE_MANAGEMENT
        UID                     = 1.2.840.10008.5.1.1.26
        DESCRIPTION             = Print Queue Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_EVENT_REPORT_RQ
        COMMAND_2               = N_EVENT_REPORT_RSP
        COMMAND_3               = N_ACTION_RQ
        COMMAND_4               = N_ACTION_RSP
        COMMAND_5               = N_GET_RQ
        COMMAND_6               = N_GET_RSP


[0086]
        NAME                    = PRINTER
        UID                     = 1.2.840.10008.5.1.1.16
        DESCRIPTION             = Printer SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_EVENT_REPORT_RQ
        COMMAND_2               = N_EVENT_REPORT_RSP
        COMMAND_3               = N_GET_RQ
        COMMAND_4               = N_GET_RSP


[0087]
        NAME                    = PRINTER_CONFIGURATION
        UID                     = 1.2.840.10008.5.1.1.16.376
        DESCRIPTION             = Printer Configuration Retrieval SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_GET_RSP


[0088]
        NAME                    = PROCEDURAL_EVENT_LOGGING
        UID                     = 1.2.840.10008.1.40
        DESCRIPTION             = Procedural Event Logging SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_ACTION_RQ
        COMMAND_2               = N_ACTION_RSP


[0089]
        NAME                    = PROCEDURE_LOG
        UID                     = 1.2.840.10008.5.1.4.1.1.88.40
        DESCRIPTION             = Procedure Log Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0090]
        NAME                    = PRODUCT_CHARACTERISTICS_QUERY
        UID                     = 1.2.840.10008.5.1.4.41
        DESCRIPTION             = Product Characteristics Query
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP


[0091]
        NAME                    = PULL_PRINT_REQUEST
        UID                     = 1.2.840.10008.5.1.1.31
        DESCRIPTION             = Pull Print Request SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_ACTION_RQ
        COMMAND_4               = N_ACTION_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP


[0092]
        NAME                    = RAW_DATA
        UID                     = 1.2.840.10008.5.1.4.1.1.66
        DESCRIPTION             = Raw Data Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0093]
        NAME                    = REAL_WORLD_VALUE_MAPPING
        UID                     = 1.2.840.10008.5.1.4.1.1.67
        DESCRIPTION             = Real World Value Mapping Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0094]
        NAME                    = REFERENCED_IMAGE_BOX
        UID                     = 1.2.840.10008.5.1.1.4.2
        DESCRIPTION             = Referenced Image Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_GET_RQ
        COMMAND_2               = N_SET_RQ
        COMMAND_3               = N_SET_RSP


[0095]
        NAME                    = RESPIRATORY_WAVEFORM
        UID                     = 1.2.840.10008.5.1.4.1.1.9.6.1
        DESCRIPTION             = RESPIRATORY WAVEFORM STORAGE
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0096]
        NAME                    = RT_BEAMS_DELIVERY_INSTRUCTION
        UID                     = 1.2.840.10008.5.1.4.34.1
        DESCRIPTION             = RT Beams Delivery Instruction Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0097]
        NAME                    = RT_CONVENTIONAL_MACHINE_VERIF
        UID                     = 1.2.840.10008.5.1.4.34.2
        DESCRIPTION             = RT Conventional Machine Verification SOP
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP
        COMMAND_7               = N_ACTION_RQ
        COMMAND_8               = N_ACTION_RSP
        COMMAND_9               = N_GET_RQ
        COMMAND_10              = N_GET_RSP
        COMMAND_11              = N_EVENT_REPORT_RSP
        COMMAND_12              = N_EVENT_REPORT_RQ


[0098]
        NAME                    = RT_ION_MACHINE_VERIF
        UID                     = 1.2.840.10008.5.1.4.34.3
        DESCRIPTION             = RT ION Machine Verification SOP
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP
        COMMAND_7               = N_ACTION_RQ
        COMMAND_8               = N_ACTION_RSP
        COMMAND_9               = N_GET_RQ
        COMMAND_10              = N_GET_RSP
        COMMAND_11              = N_EVENT_REPORT_RSP
        COMMAND_12              = N_EVENT_REPORT_RQ


[0099]
        NAME                    = SC_MULTIFRAME_GRAYSCALE_BYTE
        UID                     = 1.2.840.10008.5.1.4.1.1.7.2
        DESCRIPTION             = Multi-frame Grayscale Byte Secondary Capture Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0100]
        NAME                    = SC_MULTIFRAME_GRAYSCALE_WORD
        UID                     = 1.2.840.10008.5.1.4.1.1.7.3
        DESCRIPTION             = Multi-frame Grayscale Word Secondary Capture Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0101]
        NAME                    = SC_MULTIFRAME_SINGLE_BIT
        UID                     = 1.2.840.10008.5.1.4.1.1.7.1
        DESCRIPTION             = Multi-frame Single Bit Secondary Capture Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0102]
        NAME                    = SC_MULTIFRAME_TRUE_COLOR
        UID                     = 1.2.840.10008.5.1.4.1.1.7.4
        DESCRIPTION             = Mulfi-frame True Color Secondary Capture Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0103]
        NAME                    = SEGMENTATION
        UID                     = 1.2.840.10008.5.1.4.1.1.66.4
        DESCRIPTION             = Segmentation Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0104]
        NAME                    = SPATIAL_FIDUCIALS
        UID                     = 1.2.840.10008.5.1.4.1.1.66.2
        DESCRIPTION             = Spatial Fiducials Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0105]
        NAME                    = SPATIAL_REGISTRATION
        UID                     = 1.2.840.10008.5.1.4.1.1.66.1
        DESCRIPTION             = Spatial Registration Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0106]
        NAME                    = SPECTACLE_PRESCRIPTION_REPORT
        UID                     = 1.2.840.10008.5.1.4.1.1.78.6
        DESCRIPTION             = Spectacle Prescription Report Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0107]
        NAME                    = STANDARD_BASIC_TEXT_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.11
        DESCRIPTION             = Basic Text Structured Reporting SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0108]
        NAME                    = STANDARD_BLENDING_SOFTCOPY_PS
        UID                     = 1.2.840.10008.5.1.4.1.1.11.4
        DESCRIPTION             = Blending Softcopy Presentation State Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0109]
        NAME                    = STANDARD_COLOR_SOFTCOPY_PS
        UID                     = 1.2.840.10008.5.1.4.1.1.11.2
        DESCRIPTION             = Color Softcopy Presentation State Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0110]
        NAME                    = STANDARD_COMPREHENSIVE_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.33
        DESCRIPTION             = Comprehensive Structured Reporting SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0111]
        NAME                    = STANDARD_CR
        UID                     = 1.2.840.10008.5.1.4.1.1.1
        DESCRIPTION             = Computed Radiography Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0112]
        NAME                    = STANDARD_CT
        UID                     = 1.2.840.10008.5.1.4.1.1.2
        DESCRIPTION             = CT Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0113]
        NAME                    = STANDARD_CURVE
        UID                     = 1.2.840.10008.5.1.4.1.1.9
        DESCRIPTION             = Standalone Curve Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0114]
        NAME                    = STANDARD_DX_PRESENT
        UID                     = 1.2.840.10008.5.1.4.1.1.1.1
        DESCRIPTION             = Digital X-Ray Image Storage - For Presentation
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0115]
        NAME                    = STANDARD_DX_PROCESS
        UID                     = 1.2.840.10008.5.1.4.1.1.1.1.1
        DESCRIPTION             = Digital X-Ray Image Storage - For Processing
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0116]
        NAME                    = STANDARD_ECHO
        UID                     = 1.2.840.10008.1.1
        DESCRIPTION             = Verification SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_ECHO_RQ
        COMMAND_2               = C_ECHO_RSP


[0117]
        NAME                    = STANDARD_ENCAPSULATED_PDF
        UID                     = 1.2.840.10008.5.1.4.1.1.104.1
        DESCRIPTION             = Encapsulated PDF Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0118]
        NAME                    = STANDARD_ENHANCED_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.22
        DESCRIPTION             = Enhanced Structured Reporting SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0119]
        NAME                    = STANDARD_GRAYSCALE_SOFTCOPY_PS
        UID                     = 1.2.840.10008.5.1.4.1.1.11.1
        DESCRIPTION             = Grayscale Softcopy Presentation State Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0120]
        NAME                    = STANDARD_HARDCOPY_COLOR
        UID                     = 1.2.840.10008.5.1.1.30
        DESCRIPTION             = Harcopy Color Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0121]
        NAME                    = STANDARD_HARDCOPY_GRAYSCALE
        UID                     = 1.2.840.10008.5.1.1.29
        DESCRIPTION             = Hardcopy Grayscale Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0122]
        NAME                    = STANDARD_IO_PRESENT
        UID                     = 1.2.840.10008.5.1.4.1.1.1.3
        DESCRIPTION             = Digital Intra-oral X-Ray Image Storage - For Presentation
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0123]
        NAME                    = STANDARD_IO_PROCESS
        UID                     = 1.2.840.10008.5.1.4.1.1.1.3.1
        DESCRIPTION             = Digital Intra-oral X-Ray Image Storage - For Processing
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0124]
        NAME                    = STANDARD_IVOCT_PRESENT
        UID                     = 1.2.840.10008.5.1.4.1.1.14.1
        DESCRIPTION             = IVOCT Image Storage - For Presentation
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0125]
        NAME                    = STANDARD_IVOCT_PROCESS
        UID                     = 1.2.840.10008.5.1.4.1.1.14.2
        DESCRIPTION             = IVOCT Image Storage - For Processing
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0126]
        NAME                    = STANDARD_MG_PRESENT
        UID                     = 1.2.840.10008.5.1.4.1.1.1.2
        DESCRIPTION             = Digital Mammography Image Storage - For Presentation
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0127]
        NAME                    = STANDARD_MG_PROCESS
        UID                     = 1.2.840.10008.5.1.4.1.1.1.2.1
        DESCRIPTION             = Digital Mammography Image Storage - For Processing
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0128]
        NAME                    = STANDARD_MODALITY_LUT
        UID                     = 1.2.840.10008.5.1.4.1.1.10
        DESCRIPTION             = Standalone Modality LUT Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0129]
        NAME                    = STANDARD_MR
        UID                     = 1.2.840.10008.5.1.4.1.1.4
        DESCRIPTION             = MR Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0130]
        NAME                    = STANDARD_NM
        UID                     = 1.2.840.10008.5.1.4.1.1.20
        DESCRIPTION             = Nuclear Medicine Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0131]
        NAME                    = STANDARD_NM_RETIRED
        UID                     = 1.2.840.10008.5.1.4.1.1.5
        DESCRIPTION             = Nuclear Medicine Image Storage (Retired)
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0132]
        NAME                    = STANDARD_OPHTHALMIC_16_BIT
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.5.2
        DESCRIPTION             = Ophthalmic 16 bit Photography Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0133]
        NAME                    = STANDARD_OPHTHALMIC_8_BIT
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.5.1
        DESCRIPTION             = Ophthalmic 8 bit Photography Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0134]
        NAME                    = STANDARD_OVERLAY
        UID                     = 1.2.840.10008.5.1.4.1.1.8
        DESCRIPTION             = Standalone Overlay Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0135]
        NAME                    = STANDARD_PET
        UID                     = 1.2.840.10008.5.1.4.1.1.128
        DESCRIPTION             = Positron Emission Tomography Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0136]
        NAME                    = STANDARD_PET_CURVE
        UID                     = 1.2.840.10008.5.1.4.1.1.129
        DESCRIPTION             = Standalone PET Curve Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0137]
        NAME                    = STANDARD_PRINT_STORAGE
        UID                     = 1.2.840.10008.5.1.1.27
        DESCRIPTION             = Stored Print Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0138]
        NAME                    = STANDARD_PSEUDOCOLOR_SOFTCOPY_PS
        UID                     = 1.2.840.10008.5.1.4.1.1.11.3
        DESCRIPTION             = Pseudo-Color Softcopy Presentation State Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0139]
        NAME                    = STANDARD_RT_BEAMS_TREAT
        UID                     = 1.2.840.10008.5.1.4.1.1.481.4
        DESCRIPTION             = RT Beams Treatment Record Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0140]
        NAME                    = STANDARD_RT_BRACHY_TREAT
        UID                     = 1.2.840.10008.5.1.4.1.1.481.6
        DESCRIPTION             = RT Brachy Treatment Record Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0141]
        NAME                    = STANDARD_RT_DOSE
        UID                     = 1.2.840.10008.5.1.4.1.1.481.2
        DESCRIPTION             = RT Dose Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0142]
        NAME                    = STANDARD_RT_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.481.1
        DESCRIPTION             = RT Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0143]
        NAME                    = STANDARD_RT_ION_BEAMS_TREAT
        UID                     = 1.2.840.10008.5.1.4.1.1.481.9
        DESCRIPTION             = RT Ion Beams Treatment Record Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0144]
        NAME                    = STANDARD_RT_ION_PLAN
        UID                     = 1.2.840.10008.5.1.4.1.1.481.8
        DESCRIPTION             = RT Ion Plan Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0145]
        NAME                    = STANDARD_RT_PLAN
        UID                     = 1.2.840.10008.5.1.4.1.1.481.5
        DESCRIPTION             = RT Plan Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0146]
        NAME                    = STANDARD_RT_STRUCTURE_SET
        UID                     = 1.2.840.10008.5.1.4.1.1.481.3
        DESCRIPTION             = RT Structure Set Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0147]
        NAME                    = STANDARD_RT_TREAT_SUM
        UID                     = 1.2.840.10008.5.1.4.1.1.481.7
        DESCRIPTION             = RT Treatment Summary Record Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0148]
        NAME                    = STANDARD_SEC_CAPTURE
        UID                     = 1.2.840.10008.5.1.4.1.1.7
        DESCRIPTION             = Secondary Capture Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0149]
        NAME                    = STANDARD_US
        UID                     = 1.2.840.10008.5.1.4.1.1.6.1
        DESCRIPTION             = Ultrasound Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0150]
        NAME                    = STANDARD_US_MF
        UID                     = 1.2.840.10008.5.1.4.1.1.3.1
        DESCRIPTION             = Ultrasound Multi-Frame Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0151]
        NAME                    = STANDARD_US_MF_RETIRED
        UID                     = 1.2.840.10008.5.1.4.1.1.3
        DESCRIPTION             = Ultrasound Multi-Frame Image Storage (Retired)
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0152]
        NAME                    = STANDARD_US_RETIRED
        UID                     = 1.2.840.10008.5.1.4.1.1.6
        DESCRIPTION             = Ultrasound Image Storage (Retired)
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0153]
        NAME                    = STANDARD_VIDEO_ENDOSCOPIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.1.1
        DESCRIPTION             = Video Endoscopic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0154]
        NAME                    = STANDARD_VIDEO_MICROSCOPIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.2.1
        DESCRIPTION             = Video Microscopic Image Stroage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0155]
        NAME                    = STANDARD_VIDEO_PHOTOGRAPHIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.4.1
        DESCRIPTION             = Video Photographic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0156]
        NAME                    = STANDARD_VL_ENDOSCOPIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.1
        DESCRIPTION             = VL Endoscopic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0157]
        NAME                    = STANDARD_VL_MICROSCOPIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.2
        DESCRIPTION             = VL Microscopic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0158]
        NAME                    = STANDARD_VL_PHOTOGRAPHIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.4
        DESCRIPTION             = VL Photographic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0159]
        NAME                    = STANDARD_VL_SLIDE_MICROSCOPIC
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.3
        DESCRIPTION             = VL Slide-Coordinates Microscopic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0160]
        NAME                    = STANDARD_VOI_LUT
        UID                     = 1.2.840.10008.5.1.4.1.1.11
        DESCRIPTION             = Standalone VOI LUT Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RSP
        COMMAND_2               = C_STORE_RQ


[0161]
        NAME                    = STANDARD_WAVEFORM_12_LEAD_ECG
        UID                     = 1.2.840.10008.5.1.4.1.1.9.1.1
        DESCRIPTION             = 12-lead ECG Waveform Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0162]
        NAME                    = STANDARD_WAVEFORM_AMBULATORY_ECG
        UID                     = 1.2.840.10008.5.1.4.1.1.9.1.3
        DESCRIPTION             = Ambulatory ECG Waveform Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0163]
        NAME                    = STANDARD_WAVEFORM_BASIC_VOICE_AU
        UID                     = 1.2.840.10008.5.1.4.1.1.9.4.1
        DESCRIPTION             = Basic Voice Audio Waveform Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0164]
        NAME                    = STANDARD_WAVEFORM_CARDIAC_EP
        UID                     = 1.2.840.10008.5.1.4.1.1.9.3.1
        DESCRIPTION             = Cardiac Electrophysiology Waveform Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0165]
        NAME                    = STANDARD_WAVEFORM_GENERAL_ECG
        UID                     = 1.2.840.10008.5.1.4.1.1.9.1.2
        DESCRIPTION             = General ECG Waveform Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0166]
        NAME                    = STANDARD_WAVEFORM_HEMODYNAMIC
        UID                     = 1.2.840.10008.5.1.4.1.1.9.2.1
        DESCRIPTION             = Hemodynamic Waveform Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0167]
        NAME                    = STANDARD_XRAY_ANGIO
        UID                     = 1.2.840.10008.5.1.4.1.1.12.1
        DESCRIPTION             = X-Ray Angiographic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0168]
        NAME                    = STANDARD_XRAY_ANGIO_BIPLANE
        UID                     = 1.2.840.10008.5.1.4.1.1.12.3
        DESCRIPTION             = X-Ray Angiographic Bi-Plane Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0169]
        NAME                    = STANDARD_XRAY_RF
        UID                     = 1.2.840.10008.5.1.4.1.1.12.2
        DESCRIPTION             = X-Ray Radiofluoroscopic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0170]
        NAME                    = STEREOMETRIC_RELATIONSHIP
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.5.3
        DESCRIPTION             = Stereometric Relationship Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0171]
        NAME                    = STORAGE_COMMITMENT_PULL
        UID                     = 1.2.840.10008.1.20.2
        DESCRIPTION             = Storage Commitment Pull Model SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_ACTION_RQ
        COMMAND_2               = N_ACTION_RSP
        COMMAND_3               = N_EVENT_REPORT_RQ
        COMMAND_4               = N_EVENT_REPORT_RSP


[0172]
        NAME                    = STORAGE_COMMITMENT_PUSH
        UID                     = 1.2.840.10008.1.20.1
        DESCRIPTION             = Storage Commitment Push Model SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_ACTION_RQ
        COMMAND_2               = N_ACTION_RSP
        COMMAND_3               = N_EVENT_REPORT_RQ
        COMMAND_4               = N_EVENT_REPORT_RSP


[0173]
        NAME                    = STUDY_COMPONENT_MANAGEMENT
        UID                     = 1.2.840.10008.3.1.2.3.2
        DESCRIPTION             = Study Component Management SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_GET_RQ
        COMMAND_6               = N_GET_RSP


[0174]
        NAME                    = STUDY_CONTENT_NOTIFICATION
        UID                     = 1.2.840.10008.1.9
        DESCRIPTION             = Basic Study Content Notification SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0175]
        NAME                    = STUDY_ROOT_QR_FIND
        UID                     = 1.2.840.10008.5.1.4.1.2.2.1
        DESCRIPTION             = Study Root Query/Retrieve Information Model - FIND
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_FIND_RQ
        COMMAND_3               = C_FIND_RSP


[0176]
        NAME                    = STUDY_ROOT_QR_GET
        UID                     = 1.2.840.10008.5.1.4.1.2.2.3
        DESCRIPTION             = Study Root Query/Retrieve Information Model - GET
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_GET_RQ
        COMMAND_3               = C_GET_RSP


[0177]
        NAME                    = STUDY_ROOT_QR_MOVE
        UID                     = 1.2.840.10008.5.1.4.1.2.2.2
        DESCRIPTION             = Study Root Query/Retrieve Information Model - MOVE
        TYPE                    = BASE
        COMMAND_1               = C_CANCEL_RQ
        COMMAND_2               = C_MOVE_RQ
        COMMAND_3               = C_MOVE_RSP


[0178]
        NAME                    = SUBJ_REFRACTION_MEASUREMENTS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.4
        DESCRIPTION             = Subjective Refraction Measurements Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0179]
        NAME                    = SUBSTANCE_ADMIN_LOGGING
        UID                     = 1.2.840.10008.1.42
        DESCRIPTION             = Substance Administration Logging
        TYPE                    = BASE
        COMMAND_1               = N_ACTION_RQ
        COMMAND_2               = N_ACTION_RSP


[0180]
        NAME                    = SUBSTANCE_APPROVAL_QUERY
        UID                     = 1.2.840.10008.5.1.4.42
        DESCRIPTION             = Substance Approval Query
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP


[0181]
        NAME                    = SURFACE_SEGMENTATION
        UID                     = 1.2.840.10008.5.1.4.1.1.66.5
        DESCRIPTION             = Surface Segmentation Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0182]
        NAME                    = UPS_EVENT_SOP
        UID                     = 1.2.840.10008.5.1.4.34.4.4
        DESCRIPTION             = Unified Procedure Step EVENT SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_EVENT_REPORT_RQ
        COMMAND_2               = N_EVENT_REPORT_RSP


[0183]
        NAME                    = UPS_PULL_SOP
        UID                     = 1.2.840.10008.5.1.4.34.4.3
        DESCRIPTION             = Unified Procedure Step PULL SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_FIND_RQ
        COMMAND_2               = C_FIND_RSP
        COMMAND_3               = N_GET_RQ
        COMMAND_4               = N_GET_RSP
        COMMAND_5               = N_SET_RQ
        COMMAND_6               = N_SET_RSP
        COMMAND_7               = N_ACTION_RQ
        COMMAND_8               = N_ACTION_RSP


[0184]
        NAME                    = UPS_PUSH_SOP
        UID                     = 1.2.840.10008.5.1.4.34.4.1
        DESCRIPTION             = Unified Procedure Step PUSH SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_ACTION_RQ
        COMMAND_3               = N_CREATE_RSP
        COMMAND_4               = N_ACTION_RSP


[0185]
        NAME                    = UPS_WATCH_SOP
        UID                     = 1.2.840.10008.5.1.4.34.4.2
        DESCRIPTION             = Unified Procedure Step WATCH SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_ACTION_RQ
        COMMAND_2               = N_ACTION_RSP
        COMMAND_3               = N_GET_RQ
        COMMAND_4               = N_GET_RSP
        COMMAND_5               = C_FIND_RQ
        COMMAND_6               = C_FIND_RSP


[0186]
        NAME                    = VISUAL_ACUITY_MEASUREMENTS
        UID                     = 1.2.840.10008.5.1.4.1.1.78.5
        DESCRIPTION             = Visual Acuity Measurements Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0187]
        NAME                    = VL_WHOLE_SLIDE_MICROSCOPY_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.77.1.6
        DESCRIPTION             = VL Whole Slide Microscopy Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0188]
        NAME                    = VOI_LUT_BOX
        UID                     = 1.2.840.10008.5.1.1.22
        DESCRIPTION             = VOI LUT Box SOP Class
        TYPE                    = BASE
        COMMAND_1               = N_CREATE_RQ
        COMMAND_2               = N_CREATE_RSP
        COMMAND_3               = N_SET_RQ
        COMMAND_4               = N_SET_RSP
        COMMAND_5               = N_DELETE_RQ
        COMMAND_6               = N_DELETE_RSP


[0189]
        NAME                    = XA_XRF_GRAYSCALE_SOFTCOPY_PS
        UID                     = 1.2.840.10008.5.1.4.1.1.11.5
        DESCRIPTION             = XA/XRF Grayscale Softcopy Presentation State Storage SOP Class
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0190]
        NAME                    = XRAY_3D_ANGIO_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.13.1.1
        DESCRIPTION             = X-Ray 3D Angiographic Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0191]
        NAME                    = XRAY_3D_CRANIO_IMAGE
        UID                     = 1.2.840.10008.5.1.4.1.1.13.1.2
        DESCRIPTION             = X-Ray 3D Craniofacial Image Storage
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0192]
        NAME                    = XRAY_RADATION_DOSE_SR
        UID                     = 1.2.840.10008.5.1.4.1.1.88.67
        DESCRIPTION             = X-Ray Radiation Dose SR
        TYPE                    = BASE
        COMMAND_1               = C_STORE_RQ
        COMMAND_2               = C_STORE_RSP


[0193]
        NAME                    = BASIC_COLOR_PRINT_MANAGEMENT
        DESCRIPTION             = Basic Color Print Management Meta SOP Class
        UID                     = 1.2.840.10008.5.1.1.18
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 4
        SOP_CLASS_1             = 0004
        SOP_CLASS_2             = 0006
        SOP_CLASS_3             = 0086
        SOP_CLASS_4             = 0005


[0194]
        NAME                    = BASIC_GRAYSCALE_PRINT_MANAGEMENT
        DESCRIPTION             = Basic Grayscale Print Management Meta SOP Class
        UID                     = 1.2.840.10008.5.1.1.9
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 4
        SOP_CLASS_1             = 0086
        SOP_CLASS_2             = 0005
        SOP_CLASS_3             = 0006
        SOP_CLASS_4             = 0007


[0195]
        NAME                    = DETACHED_PATIENT_MANAGEMENT_META
        DESCRIPTION             = Detatched Patient Management Meta SOP Class
        UID                     = 1.2.840.10008.3.1.2.1.4
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 2
        SOP_CLASS_1             = 0027
        SOP_CLASS_2             = 0024


[0196]
        NAME                    = DETACHED_RESULTS_MANAGEMENT_META
        DESCRIPTION             = Detatched Results Management Meta SOP Class
        UID                     = 1.2.840.10008.3.1.2.5.4
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 2
        SOP_CLASS_1             = 0025
        SOP_CLASS_2             = 0023


[0197]
        NAME                    = G_P_WORKLIST_MANAGEMENT_META
        DESCRIPTION             = General Purpose Worklist Managment Meta SOP Class
        UID                     = 1.2.840.10008.5.1.4.32
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 3
        SOP_CLASS_1             = 0037
        SOP_CLASS_2             = 0039
        SOP_CLASS_3             = 0038


[0198]
        NAME                    = PULL_STORED_PRINT_MANAGEMENT
        DESCRIPTION             = Pull Stored Print Management Meta SOP Class
        UID                     = 1.2.840.10008.5.1.1.32
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 2
        SOP_CLASS_1             = 0086
        SOP_CLASS_2             = 0091


[0199]
        NAME                    = REF_COLOR_PRINT_MANAGEMENT
        DESCRIPTION             = Referenced Color Print Management Meta SOP Class
        UID                     = 1.2.840.10008.5.1.1.18.1
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 4
        SOP_CLASS_1             = 0086
        SOP_CLASS_2             = 0094
        SOP_CLASS_3             = 0006
        SOP_CLASS_4             = 0005


[0200]
        NAME                    = REF_GRAYSCALE_PRINT_MANAGEMENT
        DESCRIPTION             = Referenced Grayscale Print Management Meta SOP Class
        UID                     = 1.2.840.10008.5.1.1.9.1
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 5
        SOP_CLASS_1             = 0006
        SOP_CLASS_2             = 0005
        SOP_CLASS_3             = 0188
        SOP_CLASS_4             = 0094
        SOP_CLASS_5             = 0086


[0201]
        NAME                    = STUDY_MANAGEMENT
        DESCRIPTION             = Detatched Study Management Meta SOP Class
        UID                     = 1.2.840.10008.3.1.2.5.5
        TYPE                    = META
        SOP_CLASSES_INCLUDED    = 2
        SOP_CLASS_1             = 0026
        SOP_CLASS_2             = 0173


[ITEM_TABLE]
    NUMBER_OF_ITEMS_SUPPORTED             = 709
    2D_DEGREE_OF_FREEDOM                  = 0001
    2D_LINE_COORDINATES                   = 0002
    2D_MATING_FEATURE_COORDINATES         = 0003
    2D_PLANE_COORDINATES                  = 0004
    2D_POINT_COORDINATES                  = 0005
    ACQUISITION_CONTEXT                   = 0006
    ACTUAL_HUMAN_PERFORMERS               = 0007
    ACTUAL_HUMAN_PERFORMERS_N_SET         = 0008
    ADD_NEAR_SQ                           = 0009
    AGE_CORRECTED_SENSIT_DEV_ALG          = 0010
    ALGORITHM_IDENT_MACRO                 = 0011
    ALTERNATE_CONTAINER_IDENTIFIER        = 0012
    ALTERNATE_CONTENT_DESCRIPTION         = 0013
    ALTERNATE_REPRESENTATION              = 0014
    ANATOMIC_REGION                       = 0015
    ANNOTATION_CONTENT                    = 0016
    ANTERIOR_CHAMBER_DEPTH                = 0017
    APPLICATION_SETUP                     = 0018
    APPLICATOR                            = 0019
    APPLICATOR_GEOMETRY                   = 0020
    APPLICATOR_IN_ION                     = 0021
    ASL_BOLUS_CUT_OFF_TIMING              = 0022
    ASL_SLAB                              = 0023
    ASSIGNING_FACILITY                    = 0024
    ATTRIBUTE_OCCURRENCE_SQ               = 0025
    AUTHOR_OBSERVER                       = 0026
    AUTOREFRACTION_EYE_SQ                 = 0027
    BEAM_ITEM                             = 0028
    BEAM_LIMITING_DEVICE                  = 0029
    BEAM_LIMITING_DEVICE_IN_BEAM          = 0030
    BEAM_LIMITING_DEVICE_LEAF_PAIRS       = 0031
    BEAM_LIMITING_DEVICE_POSITION         = 0032
    BEAM_LIMITING_DEVICE_TOLERANCE        = 0033
    BEAM_TASK_SQ                          = 0034
    BILLING_SUPPLIES_AND_DEVICES          = 0035
    BIPLANE_ACQUISITION                   = 0036
    BLENDING_LUT_1_SQ                     = 0037
    BLENDING_LUT_2_SQ                     = 0038
    BLENDING_SEQUENCE                     = 0039
    BLOCK_SEQUENCE                        = 0040
    BRACHY_ACCESSORY_DEVICE               = 0041
    BRACHY_CONTROL_POINT                  = 0042
    BRACHY_CONTROL_POINT_DELIVERED        = 0043
    BRACHY_REFERENCED_DOSE_REFERENCE      = 0044
    BREED_REGISTRATION                    = 0045
    CALCULATED_DOSE_REFERENCE             = 0046
    CALIBRATION                           = 0047
    CALIBRATION_DATA                      = 0048
    CARDIAC_TRIGGER                       = 0049
    CHANNEL                               = 0050
    CHANNEL_DEFINITION                    = 0051
    CHANNEL_DISPLAY                       = 0052
    CHANNEL_SHIELD                        = 0053
    CHEMICAL_SHIFT                        = 0054
    CODE_SEQUENCE_MACRO                   = 0055
    CODING_SCHEME_IDENTIFICATION          = 0056
    COLLIMATOR_SHAPE                      = 0057
    COMPENSATOR                           = 0058
    COMPONENT                             = 0059
    COMPONENT_ASSEMBLY                    = 0060
    COMPONENT_TYPES                       = 0061
    COMPOUND_GRAPHIC                      = 0062
    CONCEPT_CODE_SEQUENCE                 = 0063
    CONCEPT_NAME_CODE_SEQUENCE            = 0064
    CONSENT_FOR_CLINICAL_TRIAL_USE        = 0065
    CONTAINER_COMPONENT                   = 0066
    CONTENT                               = 0067
    CONTENT_ITEM_MACRO                    = 0068
    CONTENT_TEMPLATE                      = 0069
    CONTOUR_IMAGE                         = 0070
    CONTOUR_ITEM                          = 0071
    CONTRAST_ADMIN_PROFILE                = 0072
    CONTRAST_BOLUS_ADMIN_ROUTE            = 0073
    CONTRAST_BOLUS_USAGE                  = 0074
    CONTRIBUTING_EQUIPMENT                = 0075
    CONTRIBUTING_SOP_INSTANCE_REF         = 0076
    CONTRIBUTING_SOURCES_ANGIO            = 0077
    CONTRIBUTING_SOURCES_CRANIO           = 0078
    CONTRIBUTING_SOURCES_TOMO             = 0079
    CONTROL_POINT                         = 0080
    CONTROL_POINT_DELIVERY                = 0081
    CONVENT_CONTROL_POINT_VERIF_SQ        = 0082
    CONVENT_MACHINE_VERIF_SQ              = 0083
    CORRECTED_PARAMETERS                  = 0084
    CT_ACQUISITION_DETAILS                = 0085
    CT_ACQUISITION_TYPE                   = 0086
    CT_ADDITIONAL_XRAY_SOURCE             = 0087
    CT_EXPOSURE                           = 0088
    CT_GEOMETRY                           = 0089
    CT_IMAGE_FRAME_TYPE                   = 0090
    CT_PIXEL_VALUE_TRANSFORMATION         = 0091
    CT_POSITION                           = 0092
    CT_RECONSTRUCTION                     = 0093
    CT_TABLE_DYNAMICS                     = 0094
    CT_XRAY_DETAILS                       = 0095
    CTDI_PHANTOM_TYPE_CODE                = 0096
    CUSTODIAL_ORGANIZATION                = 0097
    CYLINDER_SQ                           = 0098
    DATA_FRAME_ASSIGNMENT_SQ              = 0099
    DATA_INFO                             = 0100
    DATA_OBSERVATION                      = 0101
    DEFORMABLE_REG_GRID                   = 0102
    DEFORMABLE_REGISTRATION               = 0103
    DELIVERY_VERIF_IMAGE_SQ               = 0104
    DERIVATION_CODE                       = 0105
    DERIVATION_IMAGE                      = 0106
    DETECTOR_INFO                         = 0107
    DEVICE                                = 0108
    DIFFUSION_B_MATRIX                    = 0109
    DIFFUSION_GRADIENT                    = 0110
    DIGITAL_SIGNATURES                    = 0111
    DIMENSION_INDEX                       = 0112
    DIMENSION_ORGANIZATION                = 0113
    DIR_REC_CURVE                         = 0114
    DIR_REC_ENCAP_DOC                     = 0115
    DIR_REC_FIDUCIAL                      = 0116
    DIR_REC_FILM_BOX                      = 0117
    DIR_REC_FILM_SESSION                  = 0118
    DIR_REC_HANGING_PROTOCOL              = 0119
    DIR_REC_HL7_STRUC_DOC                 = 0120
    DIR_REC_IMAGE                         = 0121
    DIR_REC_IMAGE_BOX                     = 0122
    DIR_REC_IMPLANT                       = 0123
    DIR_REC_IMPLANT_ASSY                  = 0124
    DIR_REC_IMPLANT_GROUP                 = 0125
    DIR_REC_INTERPRETATION                = 0126
    DIR_REC_KEY_OBJECT_DOC                = 0127
    DIR_REC_MEASUREMENT                   = 0128
    DIR_REC_MODALITY_LUT                  = 0129
    DIR_REC_MRDR                          = 0130
    DIR_REC_OVERLAY                       = 0131
    DIR_REC_PALETTE                       = 0132
    DIR_REC_PATIENT                       = 0133
    DIR_REC_PRESENTATION                  = 0134
    DIR_REC_PRINT_QUEUE                   = 0135
    DIR_REC_PRIVATE                       = 0136
    DIR_REC_RAW_DATA                      = 0137
    DIR_REC_REGISTRATION                  = 0138
    DIR_REC_RESULTS                       = 0139
    DIR_REC_RT_DOSE                       = 0140
    DIR_REC_RT_PLAN                       = 0141
    DIR_REC_RT_STRUCTURE_SET              = 0142
    DIR_REC_RT_TREAT_RECORD               = 0143
    DIR_REC_SERIES                        = 0144
    DIR_REC_SPECTROSCOPY                  = 0145
    DIR_REC_SR_DOCUMENT                   = 0146
    DIR_REC_STEREOMETRIC                  = 0147
    DIR_REC_STORED_PRINT                  = 0148
    DIR_REC_STUDY                         = 0149
    DIR_REC_STUDY_COMPONENT               = 0150
    DIR_REC_SURFACE                       = 0151
    DIR_REC_TOPIC                         = 0152
    DIR_REC_VALUE_MAP                     = 0153
    DIR_REC_VISIT                         = 0154
    DIR_REC_VOI_LUT                       = 0155
    DIR_REC_WAVEFORM                      = 0156
    DISCHARGE_DIAGNOSIS_CODE              = 0157
    DISPLAY_SETS                          = 0158
    DISPLAY_SHUTTER_MACRO                 = 0159
    DISPLAYED_AREA_SELECTION              = 0160
    DOSE_REFERENCE                        = 0161
    DVH                                   = 0162
    DVH_REF_ROI                           = 0163
    DX_PATIENT_ORIENTATION_CODE           = 0164
    DX_PRIMARY_ANATOMIC_STRUCTURE         = 0165
    ELECTRON_APPLICATOR                   = 0166
    ENCRYPTED_ATTRIBUTES                  = 0167
    ENERGY_WINDOW_INFO                    = 0168
    ENERGY_WINDOW_RANGE                   = 0169
    ENHANCED_CONTRAST_BOLUS_AGENT         = 0170
    ENHANCED_PALETTE_COLOR_TABLE_SQ       = 0171
    EQUIVALENT_CDA_DOC                    = 0172
    EVENT_TIMER_SQ                        = 0173
    EXCLUDED_INTERVALS_SQ                 = 0174
    EXPOSURE_CONTROL_SENSING_REGIONS      = 0175
    EXPOSURE_DOSE                         = 0176
    EXPOSURE_SEQUENCE                     = 0177
    FAILED_ATTRIBUTES_SQ                  = 0178
    FAILED_SOP                            = 0179
    FAILED_SOP_MEDIA_CREATION             = 0180
    FIDUCIAL                              = 0181
    FIDUCIAL_SET                          = 0182
    FIELD_OF_VIEW                         = 0183
    FILL_STYLE                            = 0184
    FILM_BOX_CONTENT                      = 0185
    FILM_CONSUMPTION                      = 0186
    FILTER_OPERATIONS                     = 0187
    FIXATION                              = 0188
    FIXATION_DEVICE                       = 0189
    FLUENCE_MAP                           = 0190
    FRACTION_GROUP                        = 0191
    FRACTION_GROUP_SUMMARY                = 0192
    FRACTION_STATUS_SUMMARY               = 0193
    FRAME_ACQUISITION                     = 0194
    FRAME_ANATOMY                         = 0195
    FRAME_CONTENT_SEQ                     = 0196
    FRAME_DETECTOR_PARAMETERS             = 0197
    FRAME_DISPLAY                         = 0198
    FRAME_DISPLAY_SHUTTER                 = 0199
    FRAME_EXTRACTION                      = 0200
    FRAME_OF_REFERENCE_RELATIONSHIP       = 0201
    FRAME_PIXEL_DATA_PROPERTIES           = 0202
    FRAME_PIXEL_INTENSITY_REL_LUT         = 0203
    FRAME_PIXEL_SHIFT                     = 0204
    FRAME_VOI_LUT                         = 0205
    FRAME_VOI_LUT_WITH_LUT                = 0206
    FUNC_GROUP_BREAST_TOMO_FRAME          = 0207
    FUNC_GROUP_BREAST_TOMO_SHARE          = 0208
    FUNC_GROUP_ENHANCED_CT_FRAME          = 0209
    FUNC_GROUP_ENHANCED_CT_SHARE          = 0210
    FUNC_GROUP_ENHANCED_MR_FRAME          = 0211
    FUNC_GROUP_ENHANCED_MR_SHARE          = 0212
    FUNC_GROUP_ENHANCED_PET_FRAME         = 0213
    FUNC_GROUP_ENHANCED_PET_SHARE         = 0214
    FUNC_GROUP_ENHANCED_US_VOL_FRAME      = 0215
    FUNC_GROUP_ENHANCED_US_VOL_SHARE      = 0216
    FUNC_GROUP_ENHANCED_XA_FRAME          = 0217
    FUNC_GROUP_ENHANCED_XA_SHARE          = 0218
    FUNC_GROUP_ENHANCED_XRF_FRAME         = 0219
    FUNC_GROUP_ENHANCED_XRF_SHARE         = 0220
    FUNC_GROUP_IVOCT_FRAME                = 0221
    FUNC_GROUP_IVOCT_SHARE                = 0222
    FUNC_GROUP_MR_SPECTROSCOPY_FRAME      = 0223
    FUNC_GROUP_MR_SPECTROSCOPY_SHARE      = 0224
    FUNC_GROUP_OPHTHALMIC_TOMO_FRAME      = 0225
    FUNC_GROUP_OPHTHALMIC_TOMO_SHARE      = 0226
    FUNC_GROUP_SECONDARY_CAPTURE          = 0227
    FUNC_GROUP_SEGMENTATION_FRAME         = 0228
    FUNC_GROUP_SEGMENTATION_SHARE         = 0229
    FUNC_GROUP_VL_WH_SL_MICRO_FRAME       = 0230
    FUNC_GROUP_VL_WH_SL_MICRO_SHARE       = 0231
    FUNC_GROUP_XRAY_3D_ANGIO_FRAME        = 0232
    FUNC_GROUP_XRAY_3D_ANGIO_SHARE        = 0233
    FUNC_GROUP_XRAY_3D_CRANIO_FRAME       = 0234
    FUNC_GROUP_XRAY_3D_CRANIO_SHARE       = 0235
    GATED_INFO                            = 0236
    GENERAL_ACCESSORY                     = 0237
    GENERAL_MACHINE_VERIF_SQ              = 0238
    GENERALIZD_DEFECT_SENSIT_DEV_ALG      = 0239
    GLOBAL_DEVIATION_PROBABILITY          = 0240
    GRAPHIC_ANNOTATION                    = 0241
    GRAPHIC_COORDINATES_DATA              = 0242
    GRAPHIC_GROUP                         = 0243
    GRAPHIC_LAYER                         = 0244
    GRAPHIC_OBJECT                        = 0245
    HANGING_PROTOCOL_DEFINITION           = 0246
    HIERARCHICAL_SERIES_REF_MACRO         = 0247
    HIERARCHICAL_SOP_INST_REF_MACRO       = 0248
    HISTOGRAM                             = 0249
    HL7_HIERARCHIC_DESIGNATOR_MACRO       = 0250
    HL7_STRUCT_DOC_REF                    = 0251
    HPGL_DOCUMENT                         = 0252
    HPGL_PEN                              = 0253
    ICON_IMAGE                            = 0254
    IDENTICAL_DOCUMENTS                   = 0255
    IDENTIFIED_PERSON_DEVICE_MACRO        = 0256
    IMAGE_BOX_CONTENT                     = 0257
    IMAGE_BOX_SYNCHRONIZATION             = 0258
    IMAGE_BOXES                           = 0259
    IMAGE_CENTER_POINT_COORDINATES        = 0260
    IMAGE_DATA_TYPE_SQ                    = 0261
    IMAGE_OVERLAY_BOX_CONTENT             = 0262
    IMAGE_PIXEL_MACRO                     = 0263
    IMAGE_SEGMENT                         = 0264
    IMAGE_SET_SELECTOR                    = 0265
    IMAGE_SETS                            = 0266
    IMAGE_SOP_INSTANCE_REF_MACRO          = 0267
    IMPLANT_ASSMBLY_TMPL_TARGET_ANAT      = 0268
    IMPLANT_TARGET_ANATOMY                = 0269
    IMPLANT_TEMPLATE_GROUP_MEMBERS        = 0270
    IMPLANT_TEMPLATE_GRP_TARGET_ANAT      = 0271
    IMPLANT_TEMPLATE_GRP_VAR_DIM_RNK      = 0272
    IMPLANT_TEMPLATE_GRP_VAR_DIMENS       = 0273
    IMPLANT_TEMPLATE_GRPMM_2D_COORDS      = 0274
    INDEX_PROBABILITY                     = 0275
    INFORMATION_FROM_MANUFACTURER         = 0276
    INTERPRETATION_APPROVER               = 0277
    INTERPRETATION_DIAGNOSIS_CODES        = 0278
    INTERV_DRUG_INFO                      = 0279
    INTERVENTIONAL_THERAPY                = 0280
    INTRAOCULAR_LENS_CALC_LEFT_EYE        = 0281
    INTRAOCULAR_LENS_CALC_RIGHT_EYE       = 0282
    IOL_POWER                             = 0283
    ION_BEAM                              = 0284
    ION_BEAM_LIMITING_DEVICE              = 0285
    ION_BLOCK                             = 0286
    ION_CONTROL_POINT                     = 0287
    ION_CONTROL_POINT_DELIVERY            = 0288
    ION_CONTROL_POINT_VERIF_SQ            = 0289
    ION_MACHINE_VERIF_SQ                  = 0290
    ION_RANGE_COMPENSATOR                 = 0291
    ION_TOLERANCE_TABLE                   = 0292
    ION_WEDGE                             = 0293
    ION_WEDGE_POSITION                    = 0294
    IRRADIATION_EVENT_ID                  = 0295
    ISOCENTER_REFERENCE_SYSTEM            = 0296
    ISSUER_OF_ACCESSION_NUMBER            = 0297
    ISSUER_PATIENT_ID_QUALIFIERS          = 0298
    IV_FRAME_CONTENT_SEQ                  = 0299
    IVOCT_FRAME_CONTENT_SEQ               = 0300
    IVOCT_FRAME_TYPE                      = 0301
    KERATOMETRIC_AXIS_SQ                  = 0302
    KERATOMETRY_EYE_SQ                    = 0303
    KERATOMETRY_MEAS_TYPE_CODE            = 0304
    LANGUAGE_CODE_RQ                      = 0305
    LANGUAGE_CODE_RSP                     = 0306
    LATERAL_SPREADING_DEVICE              = 0307
    LATERAL_SPREADING_DEVICE_SETTING      = 0308
    LENS_CONSTANT                         = 0309
    LENS_SQ                               = 0310
    LENS_THICKNESS                        = 0311
    LIGHT_PATH_FILTER_TYPE_STACK          = 0312
    LINE_STYLE                            = 0313
    LOCALIZED_DEVIATION_PROBABILITY       = 0314
    MAC_PARAMETERS                        = 0315
    MAJOR_TICKS                           = 0316
    MASK_FRAME_PIXEL_SHIFT                = 0317
    MASK_SUBTRACTION                      = 0318
    MASK_SUBTRACTION_IN_PS                = 0319
    MATING_FEATURE                        = 0320
    MATING_FEATURE_DEGREE_OF_FREEDOM      = 0321
    MATING_FEATURE_SETS                   = 0322
    MATRIX                                = 0323
    MATRIX_REGISTRATION                   = 0324
    MEASURED_DOSE_REFERENCE               = 0325
    MEASURED_VALUE                        = 0326
    MEASURING_UNITS                       = 0327
    MEDIA_INSTALLED                       = 0328
    MODALITY_LUT                          = 0329
    MODIFIED_ATTRIBUTES                   = 0330
    MR_ARTERIAL_SPIN_LABELING             = 0331
    MR_AVERAGES                           = 0332
    MR_DIFFUSION                          = 0333
    MR_ECHO                               = 0334
    MR_FOV_GEOMETRY                       = 0335
    MR_IMAGE_DESCRIPTION_MACRO            = 0336
    MR_IMAGE_FRAME_TYPE                   = 0337
    MR_IMAGING_MODIFIER                   = 0338
    MR_METABOLITE_MAP                     = 0339
    MR_MODIFIER                           = 0340
    MR_RECEIVE_COIL                       = 0341
    MR_SPATIAL_SATURATION                 = 0342
    MR_SPECTROSCOPY_FOV_GEOMETRY_MAC      = 0343
    MR_SPECTROSCOPY_FRAME_TYPE            = 0344
    MR_TIMING_RELATED_PARMS               = 0345
    MR_TRANSMIT_COIL                      = 0346
    MR_VELOCITY_ENCODING                  = 0347
    MULTI_COIL_DEFINITION                 = 0348
    MULTI_FRAME_PRESENTATION              = 0349
    MULTIPLEXED_AUDIO_CHANNELS            = 0350
    MYDRIATIC_AGENT                       = 0351
    MYDRIATIC_AGENT_CONCENTRATION         = 0352
    NAVIGATION_INDICATOR                  = 0353
    NOMINAL_SCREEN_DEFINITION             = 0354
    NOTIFICATION_FROM_MANUFACTURER        = 0355
    OBJECT_THICKNESS                      = 0356
    OPERATING_MODE                        = 0357
    OPERATOR_IDENTIFICATION               = 0358
    OPHT_AXIAL_LENGTH                     = 0359
    OPHT_AXL_LEN_MEAS_LEN_SUMMATION       = 0360
    OPHT_AXL_LEN_MEAS_SEGMENTAL_LEN       = 0361
    OPHT_AXL_LEN_MEAS_TOTAL_LEN           = 0362
    OPHT_AXL_LEN_MEASUREMENTS             = 0363
    OPHT_AXL_LEN_QUALITY_METRIC           = 0364
    OPHT_AXL_MEAS_LEFT_EYE                = 0365
    OPHT_AXL_MEAS_RIGHT_EYE               = 0366
    OPHT_PAT_CLINICAL_INFO_LEFT_EYE       = 0367
    OPHT_PAT_CLINICAL_INFO_RIGHT_EYE      = 0368
    OPHTHALMIC_FRAME_LOCATION             = 0369
    OPM_THICKNESS_MAP_NORMALS             = 0370
    OPM_THICKNESS_MAP_Q_THRESHOLD         = 0371
    OPM_THICKNESS_MAP_QR_SEQ              = 0372
    OPTICAL_OPHT_AXL_LEN_MEAS             = 0373
    OPTICAL_PATH                          = 0374
    OPTICAL_PATH_IDENTIFICATION           = 0375
    OPTICAL_SEL_OPHT_AXL_LEN              = 0376
    ORIGINAL_ATTRIBUTES                   = 0377
    ORIGINAL_IMAGE                        = 0378
    OTHER_MEDIA_AVAILABLE                 = 0379
    OTHER_PATIENT_IDS                     = 0380
    OTHER_PATIENT_IDS_N_CREATE            = 0381
    OTHER_PATIENT_IDS_N_GET_RQ            = 0382
    OTHER_PATIENT_IDS_N_GET_RSP           = 0383
    OUTPUT_INFORMATION                    = 0384
    OVERLAY_PIXEL_DATA                    = 0385
    OVERRIDE                              = 0386
    OVERRIDE_IN_RT_BRACHY_SESS            = 0387
    OVERRIDEN_ATTRIBUTES_SQ               = 0388
    PALETTE_COLOR_LOOKUP_TABLE            = 0389
    PARTICIPANT                           = 0390
    PATIENT_CLINICAL_TRIAL                = 0391
    PATIENT_GANTRY_RELATIONSHIP_CODE      = 0392
    PATIENT_ORIENTATION_CODE              = 0393
    PATIENT_ORIENTATION_IN_FRAME          = 0394
    PATIENT_PHYSIOLOGICAL_STATE           = 0395
    PATIENT_SETUP                         = 0396
    PER_PROJECTION_ACQUISITION_ANGIO      = 0397
    PER_PROJECTION_ACQUISITION_TOMO       = 0398
    PERFORMED_ACTION_ITEM                 = 0399
    PERFORMED_PROTOCOL_CODE               = 0400
    PERFORMED_SERIES                      = 0401
    PERSON_IDENTIFICATION_MACRO           = 0402
    PERTINENT_DOCUMENTS                   = 0403
    PERTINENT_DOCUMENTS_IN_SUBSTANCE      = 0404
    PET_DETECTOR_MOTION_DETAILS           = 0405
    PET_FRAME_ACQUISITION                 = 0406
    PET_FRAME_CORRECTION_FACTORS          = 0407
    PET_FRAME_TYPE                        = 0408
    PET_POSITION                          = 0409
    PET_RECONSTRACTION                    = 0410
    PET_TABLE_DYNAMICS                    = 0411
    PHASE_INFO                            = 0412
    PIXEL_INTENSITY_RELATIONSHIP_LUT      = 0413
    PIXEL_MEASURES_SEQ                    = 0414
    PIXEL_SPACING                         = 0415
    PIXEL_VALUE_MAP_TO_CODED_CONCEPT      = 0416
    PIXEL_VALUE_TRANSFORM_WITH_EV         = 0417
    PIXEL_VALUE_TRANSFORMATION            = 0418
    PLANE_ORIENTATION_SEQ                 = 0419
    PLANE_ORIENTATION_VOLUME_SQ           = 0420
    PLANE_POSITION_SEQ                    = 0421
    PLANE_POSITION_SLIDE                  = 0422
    PLANE_POSITION_VOLUME_SQ              = 0423
    PLANNED_VERIFICATION_IMAGE            = 0424
    PLANNING_LANDMARK_LINE                = 0425
    PLANNING_LANDMARK_PLANE               = 0426
    PLANNING_LANDMARK_POINT               = 0427
    POINTS_MACRO                          = 0428
    POSITIONER_POSITION                   = 0429
    POST_DEFORMATION_MATRIX_REG           = 0430
    PRE_DEFORMATION_MATRIX_REG            = 0431
    PREFORMATTED_COLOR_IMAGE              = 0432
    PREFORMATTED_GRAYSCALE_IMAGE          = 0433
    PRESENTATION_LUT                      = 0434
    PRESENTATION_LUT_CONTENT              = 0435
    PRIMARY_ANATOMIC_STRUCT_MOD           = 0436
    PRIMARY_ANATOMIC_STRUCTURE            = 0437
    PRIMARY_FLUENCE_MODE                  = 0438
    PRIMITIVE_POINT                       = 0439
    PRINT_JOB_DESCRIPTION                 = 0440
    PRINT_MANAGEMENT_CAPABILITIES         = 0441
    PRINTER_CHARACTERISTICS               = 0442
    PRINTER_CONFIGURATION                 = 0443
    PRISM_SQ                              = 0444
    PROCEDURE_TYPE_CODE_QUERY             = 0445
    PROJECTION_PIXEL_CALIBRATION          = 0446
    PROPOSED_STUDY                        = 0447
    PROTOCOL_CONTEXT                      = 0448
    QUANTITY                              = 0449
    RADIOPHARM_INFO                       = 0450
    RADIOPHARM_INFO_IN_PET                = 0451
    RADIOPHARM_INFO_PET                   = 0452
    RADIOPHARM_USAGE                      = 0453
    RANGE_MODULATOR                       = 0454
    RANGE_MODULATOR_SETTINGS              = 0455
    RANGE_SHIFTER                         = 0456
    RANGE_SHIFTER_SETTINGS                = 0457
    REAL_WORLD_VALUE_MAP_MACRO            = 0458
    REAL_WORLD_VALUE_MAPPING              = 0459
    RECORDED_BLOCK                        = 0460
    RECORDED_BRACHY_ACCESSORY_DEVICE      = 0461
    RECORDED_CHANNEL                      = 0462
    RECORDED_CHANNEL_SHIELD               = 0463
    RECORDED_COMPENSATOR                  = 0464
    RECORDED_COMPENSATOR_IN_ION           = 0465
    RECORDED_LATERAL_SPREADING_DEV        = 0466
    RECORDED_RANGE_MODULATOR              = 0467
    RECORDED_RANGE_SHIFTER                = 0468
    RECORDED_SNOUT                        = 0469
    RECORDED_SOURCE                       = 0470
    RECORDED_SOURCE_APPLICATOR            = 0471
    RECORDED_WEDGE                        = 0472
    REF_BASIC_ANNOTATION_BOX              = 0473
    REF_BEAM                              = 0474
    REF_BEAM_IN_DOSE                      = 0475
    REF_BOLUS                             = 0476
    REF_BOLUS_IN_ION                      = 0477
    REF_BRACHY_APPLICATION_SETUP          = 0478
    REF_CALCULATED_DOSE_REFERENCE         = 0479
    REF_COMPOSITE_OBJECT                  = 0480
    REF_CONTROL_POINT                     = 0481
    REF_CURVE                             = 0482
    REF_DIGITAL_SIGNATURE                 = 0483
    REF_DOSE                              = 0484
    REF_DOSE_REFERENCE                    = 0485
    REF_DOSE_REFERENCE_BEAMS              = 0486
    REF_DOSE_REFERENCE_IN_ION             = 0487
    REF_FILM_BOX                          = 0488
    REF_FILM_SESSION                      = 0489
    REF_FRACTION_GROUP                    = 0490
    REF_FRAME_OF_REFERENCE                = 0491
    REF_G_P_SCHEDULED_PROCEDURE_STEP      = 0492
    REF_IMAGE                             = 0493
    REF_IMAGE_BOX                         = 0494
    REF_IMAGE_F5-23                       = 0495
    REF_IMAGE_IN_IMAGE_BOX                = 0496
    REF_IMAGE_IN_REF_SERIES               = 0497
    REF_IMAGE_IN_STORE                    = 0498
    REF_IMAGE_OVERLAY_BOX                 = 0499
    REF_IMAGE_OVERLAY_BOX_IN_STORE        = 0500
    REF_IMAGE_REAL_WORLD_FOR_NM           = 0501
    REF_IMAGE_REAL_WORLD_VALUE_MAP        = 0502
    REF_IMAGE_RQ_F.4-3                    = 0503
    REF_IMAGE_RSP_F.4-2                   = 0504
    REF_IMAGE_RSP_F.4-3                   = 0505
    REF_IMAGE_RT                          = 0506
    REF_IMAGE_STRUCT_DISPLAY              = 0507
    REF_INSTANCE                          = 0508
    REF_INSTANCE_IN_CONTRIB               = 0509
    REF_INTERPRETATION                    = 0510
    REF_MEASURED_DOSE_REFERENCE           = 0511
    REF_OPHT_AXL_LEN_MEAS_QC_IMAGE        = 0512
    REF_OVERLAY                           = 0513
    REF_OVERLAY_IN_CURVE                  = 0514
    REF_OVERLAY_IN_IMAGE_BOX              = 0515
    REF_PATIENT                           = 0516
    REF_PATIENT_ALIAS                     = 0517
    REF_PERFORMED_PROCEDURE_STEP          = 0518
    REF_PLAN                              = 0519
    REF_PRESENTATION_LUT                  = 0520
    REF_PRESENTATION_LUT_IN_STORE         = 0521
    REF_PRINT_JOB                         = 0522
    REF_PRINT_JOB_IN_DESCRIPTION          = 0523
    REF_REAL_WORLD_VALUE_MAPPING          = 0524
    REF_REFERENCE_IMAGE                   = 0525
    REF_REFERENCE_IMAGE_IN_ION            = 0526
    REF_RESULTS                           = 0527
    REF_ROI                               = 0528
    REF_RT_PLAN                           = 0529
    REF_RT_PLAN_IN_DOSE                   = 0530
    REF_RT_SERIES                         = 0531
    REF_RT_STUDY                          = 0532
    REF_SERIES                            = 0533
    REF_SERIES_F5-23                      = 0534
    REF_SERIES_IN_COMMON_INSTANCE         = 0535
    REF_SERIES_IN_CONTRIB                 = 0536
    REF_SERIES_IN_PS                      = 0537
    REF_SERIES_NOTIFICATION               = 0538
    REF_SERIES_RQ_F.4-2                   = 0539
    REF_SERIES_RQ_F.4-3                   = 0540
    REF_SERIES_RSP_F.4-2                  = 0541
    REF_SERIES_RSP_F.4-3                  = 0542
    REF_SETUP_IMAGE                       = 0543
    REF_SOP                               = 0544
    REF_SOP_AE_RQ                         = 0545
    REF_SOP_AE_RSP                        = 0546
    REF_SOP_FOR_IMAGE_MACRO               = 0547
    REF_SOP_IN_HS_MACRO                   = 0548
    REF_SOP_INSTANCE_MAC                  = 0549
    REF_SOP_MEDIA                         = 0550
    REF_SOP_MEDIA_AE                      = 0551
    REF_SOP_MEDIA_CREATION                = 0552
    REF_SOP_NOTIFICATION                  = 0553
    REF_SOURCE                            = 0554
    REF_STORAGE_MEDIA                     = 0555
    REF_STORED_PRINT                      = 0556
    REF_STRUCTURE_SET                     = 0557
    REF_STUDY                             = 0558
    REF_STUDY_COMPONENT                   = 0559
    REF_TREATMENT_RECORD                  = 0560
    REF_VERIFICATION_IMAGE                = 0561
    REF_VISIT                             = 0562
    REF_VOI_LUT_BOX                       = 0563
    REF_WAVEFORM                          = 0564
    REFERENCED_IMAGE                      = 0565
    REFERENCED_IMAGE_NAVIGATION           = 0566
    REFERENCED_REQUEST                    = 0567
    REFERENCED_REQUEST_N_CREATE_RQ        = 0568
    REFERENCED_REQUEST_N_CREATE_RSP       = 0569
    REFERENCED_REQUEST_N_GET_RQ           = 0570
    REFERENCED_SERIES                     = 0571
    REFERENCED_SERIES_10_4                = 0572
    REFERENCED_SOP                        = 0573
    REFERENCED_SURFACE                    = 0574
    REFRACTIVE_PARAMS_USED_ON_PAT         = 0575
    REFRACTIVE_STATE                      = 0576
    REFRACTIVE_STATE_IOL                  = 0577
    REGION_PIXEL_SHIFT                    = 0578
    REGISTRATION                          = 0579
    REGISTRATION_TO_LOCALIZER_SEQ         = 0580
    REL_OPT_ATTRIBUTES_SEQ                = 0581
    RELATED_PROCEDURE_STEP_N_CREATE       = 0582
    RELATED_PROCEDURE_STEP_N_GET_RSP      = 0583
    RELATED_PROCEDURE_STEP_SQ             = 0584
    RELATED_RT_ROI_OBSERVATIONS           = 0585
    RELATED_SERIES                        = 0586
    REQUEST_ATTRIBUTES                    = 0587
    RESPIRATORY_TRIGGER                   = 0588
    RESULTS_DISTRIBUTION_LIST             = 0589
    RESULTS_NORMALS                       = 0590
    ROI_CONTOUR                           = 0591
    ROI_DENSITY                           = 0592
    ROI_ELEMENTAL_COMPOSITION             = 0593
    ROI_PHYSICAL_PROPERTIES               = 0594
    ROTATION_INFO                         = 0595
    RT_DOSE_ROI                           = 0596
    RT_MOTION_SYNCHRONIZATION             = 0597
    RT_RELATED_ROI                        = 0598
    RT_ROI_IDENTIFICATION_CODE            = 0599
    RT_ROI_OBSERVATIONS                   = 0600
    SCHED_HUMAN_PERFORMERS                = 0601
    SCHED_HUMAN_PERFORMERS_N_CREATE       = 0602
    SCHEDULED_ACTION_ITEM_CODE            = 0603
    SCHEDULED_PROCEDURE_STEP              = 0604
    SCHEDULED_PROTOCOL_CODE               = 0605
    SCHEDULED_STEP_ATTRIBUTE              = 0606
    SCREENING_BASELINE_MEASURED           = 0607
    SEGMENT                               = 0608
    SEGMENT_IDENTIFICATION                = 0609
    SELECTED_SEGMENTAL_OPHT_AXL_LEN       = 0610
    SELECTED_TOTAL_OPHT_AXL_LENGTH        = 0611
    SETUP_DEVICE                          = 0612
    SHIELDING_DEVICE                      = 0613
    SNOUT                                 = 0614
    SOFTCOPY_PRESENTATION_LUT             = 0615
    SOFTCOPY_VOI_LUT                      = 0616
    SOP_INSTANCE_REF_MACRO                = 0617
    SORTING_OPERATIONS                    = 0618
    SOURCE                                = 0619
    SOURCE_HANGING_PROTOCOL               = 0620
    SOURCE_IMAGE                          = 0621
    SOURCE_IMAGE_C_7_6_16_2_6             = 0622
    SOURCE_INSTANCE                       = 0623
    SOURCE_WAVEFORM                       = 0624
    SPECIFIC_ABSORPTION_RATE              = 0625
    SPECIMEN_DESCRIPTION                  = 0626
    SPECIMEN_DESCRIPTION_IN_IMAGE         = 0627
    SPECIMEN_IDENTIFICATION               = 0628
    SPECIMEN_MACRO                        = 0629
    SPECIMEN_PREPARATION                  = 0630
    SPECIMEN_REFERENCE                    = 0631
    SR_CONTENT                            = 0632
    SRC_OF_REFRACT_MEAS                   = 0633
    STEREO_PAIRS                          = 0634
    STRUCTURE_SET_ROI                     = 0635
    STRUCTURED_DISPLAY_IMAGE_BOX          = 0636
    STRUCTURED_DISPLAY_TEXT_BOX           = 0637
    STUDIES_CONTAIN_OTHER_REF_INST        = 0638
    SUBJECTIVE_REFRACTION_EYE             = 0639
    SUPPORTED_IMAGE_DISPLAY_FORMATS       = 0640
    SURFACE                               = 0641
    SURFACE_MESH_PR_MACRO                 = 0642
    SURFACE_MODEL_DESCRIPTION             = 0643
    SYNCHRONIZED_SCROLLING                = 0644
    TABLE_POSITION                        = 0645
    TEMPLATE_IDENTIFICATION_MACRO         = 0646
    TEMPORAL_POSITION_SQ                  = 0647
    TEST_POINT_NORMALS                    = 0648
    TEXT_OBJECT                           = 0649
    TEXT_STYLE                            = 0650
    TIME_BASED_IMAGE_SETS                 = 0651
    TIME_SLOT_INFO                        = 0652
    TOLERANCE_TABLE                       = 0653
    TOTAL_PIXEL_MATRIX_ORIGIN             = 0654
    TRANSDUCER_ORIENTATION                = 0655
    TRANSDUCER_ORIENTATION_MOD            = 0656
    TRANSDUCER_POSITION                   = 0657
    TRANSDUCER_POSITION_MOD               = 0658
    TREAT_SESSION_APPLICATION_SETUP       = 0659
    TREAT_SUM_CALCULATED_DOSE_REF         = 0660
    TREAT_SUM_MEASURED_DOSE_REF           = 0661
    TREATMENT_MACHINE                     = 0662
    TREATMENT_MACHINE_IN_TREAT            = 0663
    TREATMENT_SESSION_BEAM                = 0664
    TREATMENT_SESSION_ION_BEAM            = 0665
    ULTRASOUND_OPHT_AXL_LEN_MEAS          = 0666
    ULTRASOUND_REGION                     = 0667
    ULTRASOUND_SEL_OPHT_AXL_LEN           = 0668
    UPS_CODE_SQ                           = 0669
    UPS_CODE_SQ_N_GET                     = 0670
    UPS_COMMUNICATIONS_URI_N_SET_RQ       = 0671
    UPS_COMMUNICATIONS_URI_SQ             = 0672
    UPS_CONTENT_ITEM_MACRO                = 0673
    UPS_CONTENT_ITEM_MACRO_N_CREATE       = 0674
    UPS_PERFORMED_PROCEDURE_N_SET         = 0675
    UPS_PERFORMED_PROCEDURE_SQ            = 0676
    UPS_PROGRESS_INFO_N_SET_RSP           = 0677
    UPS_PROGRESS_INFO_SQ                  = 0678
    US_IMAGE_DESCRIPTION_SQ               = 0679
    USED_FIDUCIALS                        = 0680
    VECTORS_MACRO                         = 0681
    VELOCITY_ENCODING_ACQUISITION         = 0682
    VERIFYING_OBSERVER                    = 0683
    VIEW_CODE                             = 0684
    VIEW_CODE_BREAST                      = 0685
    VIS_FIELD_GLOBAL_RESULTS_INDEX        = 0686
    VIS_FIELD_TEST_RELI_GLOBAL_INDEX      = 0687
    VISUAL_ACUITY_EYE_SQ                  = 0688
    VISUAL_ACUITY_MEASUREMENT             = 0689
    VISUAL_FIELD_CATCH_TRIAL              = 0690
    VISUAL_FIELD_TEST_POINT               = 0691
    VISUAL_FIELD_TEST_POINT_NORMALS       = 0692
    VOI_LUT                               = 0693
    VOLUME_LOCALIZATION                   = 0694
    WAVEFORM                              = 0695
    WAVEFORM_ANNOTATION                   = 0696
    WAVEFORM_PRESENTATION_GROUP           = 0697
    WEDGE_ITEM                            = 0698
    WEDGE_POSITION                        = 0699
    X_RAY_3D_GEN_ACQ_PER_PROJ_MACRO       = 0700
    XA_XRF_FRAME_CHARACTERISTICS          = 0701
    XA_XRF_FRAME_DISPLAY_SHUTTER          = 0702
    XA_XRF_MASK_SUBTRACTION               = 0703
    XRAY_3D_ACQUISITION_ANGIO             = 0704
    XRAY_3D_ACQUISITION_CRANIO            = 0705
    XRAY_3D_ACQUISITION_TOMO              = 0706
    XRAY_3D_FRAME_TYPE                    = 0707
    XRAY_3D_RECONSTRUCTION                = 0708
    XRAY_GEOMETRY                         = 0709
